Breakdown/conditioning functions

Read in config file with parameters

Initialse RF

Set averaging for cav\_rev and cav\_fwd

Monitor traces required for breakdown data

Set masks (after / before a power increase)

Set mean trace position for klystron and cavity (fwd & rev)

Set monitoringfor continuous acq

Create and Connect up the gui

Update gui

If we can increase RF: